Making a 12 volt T Starter

1. Split fields at connection between 2 &3 with a high speed cutter
2. Cut the right side of the field winding near post between 1 & 4 leave enough material so washer has a support area
3. unsolder  fields 4 & 3
4. unsolder old lead that used to attach to 4 from the post, throw it away
5. unsolder brushes leads from fields 3 & 2, throw away old brushes leads
6. field 3, bend curled lead straight up and down
7. unwrap and rewrap windings as needed

red marks = Cutting/unsolder points

8. Swap fields 3 & 4

	
9. New lead from 4 to 2 should be too long, twist and cut to make correct distance and resolder

10. using a 2 inch piece of 1/4" smashed copper tubing connect field 4 to field 3

11. using a 1 inch piece of 1/4" smashed copper tubing, curl ends and slide over last open connection. 12. Then cut two new  brush leads long enough to reach both brush holders  
13. Slide end of new brush leads into curled tubing and solder onto open connection

Install into Case, Check for Shorts in wiring